# Kurzweil M3W v1.16 Update

8/28/17

## Files Included in this Download

> Filename | Purpose
> --- | ---
> M3W_v116_ReadMe.html | This document, detailing installation plus a history of all O/S enhancements.
> M3WV116.KUF | System update file.

## Requirements

- Mac or PC with USB port
- USB cable

## v1.16 Release Notes

1. Initial release.

## Installation

Start with the M3W's power off.

1. Press and hold down the PLAY/STOP button. Power on the M3W keeping the PLAY/STOP button depressed.
2. On the M3W screen, you will see a scrolling text displaying:

              "M3W BOOTLOADER v1.XX"

3. Once this text scrolls by once, the screen will display:

              "RUN M3W"

4. Connect a USB cable between the M3W and your computer.

   A temporary USB drive representing the M3W will mount on your computer (the drive icon may appear on your Desktop, under "Devices" (Mac) or under "My Computer" (PC).

5. Press the SELECT RIGHT (>) button twice. The screen will display:

              "UPDATE SOFTWARE"

6. Press NEXT(⊕) once. The screen will display:

              "UPDATE"

7. Press NEXT(⊕) again. The screen will display the following:

              "COPY FILE TO..."

8. On your computer, copy (drag and drop) the "M3WV116.KUF" file to the temporary USB drive.
9. Unmount or "Safely Remove" the drive from your computer.
10. Press NEXT(⊕) again on your M3W to initiate the update.
11. The screen will display:

               "UPDATING ... "

12. When complete, the screen will display:

               "UPDATED"

13. Power the M3W off then back on normally.

The update process is now complete.

-END-