# KURZWEIL Mark ProONEi OS v1.03 UPDATE

This zipped archive includes:

OS FILES | DOCUMENTS
Mark ProONEi-v103.mid ONEi boot V101.mid | Mark ProONEi-README.html Mark-Pro ONEi UpdateManual RevE (OS).pdf Mark-Pro ONEi UpdateManual RevE (Boot).pdf Mark-Pro ONEi 64voice(Quick GUIDE).pdf

## v1.03 Release Notes

1. Vista USB - compatibility added. Note: no driver required when using Vista.

Past Release Notes

## Installation

The Mark ProONEi receives its system updates through MIDI sys-ex (i.e. playing a specified MIDI file containing system exclusive data into its USB port via MIDI-over-USB.) Details on how to update your Mark ProONEi system files can be found in the Mark-Pro ONEi UpdateManual RevE (OS).pdf and Mark-Pro ONEi UpdateManual RevE (Boot).pdf (both included in this download).

Update Requirements / Recommendations

> Windows Users:
> - XP Users: to update to v1.03 via USB, simply follow the included instructions Mark-Pro ONEi UpdateManual RevE (OS).pdf . (No need to update the boot loader)

> (recommended for XP users) "Mark-Pro ONEi.inf" XP driver (available on Kurzweil's website). The installation of this driver permits your host DAW to reference the Mark ProONEi by name versus a generic, standard driver label. Unnecessary for Vista.

> - Vista Users: to update to OS v1.03 via USB, you must first update the system Boot Loader to v1.01 (file included). This must be done using XP. Follow the included installation instructions Mark-Pro ONEi UpdateManual RevE (Boot).pdf.

>   After completing the Boot Loader update, update to OS v1.03 (either XP or Vista), following the included instructions Mark-Pro ONEi UpdateManual RevE (OS).pdf .

> Mac OSX Users:
> - To update to v1.03 via USB, simply follow the included instructions Mark-Pro ONEi UpdateManual RevE (OS).pdf . (No need to update the boot loader)
> - NO OSX driver required

## Past Release Notes

- ### Version 1.02

  - adds 32 additional sounds for a total of 64 preset programs.

- ### Version 1.01

  - initial Mark ProONEi OS release

-END-